
 --CONTENTS--
 1 - SUPPORTED OPERATING SYSTEMS
 2 - UEFI Shell Installation Instructions

----------------------------------------------------------------------
SUPPORTED OPERATING SYSTEMS
----------------------------------------------------------------------
* Non-OS
* VMware
* Windows Server 2016
* RHEL 7.5  (Kernel Version:3.10)


*****************************************************************************
*              2. UEFI Shell Installation Instructions                      *
*                                                                           *
*     1.  Please make note of any settings you have changed in the BIOS     *
*         Setup utility. They may have to be re-entered after updating      *
*         the BIOS.                                                         *
*     2.  Copy "efi" folder and all files include uEFI ROM to USB disk      *
*         root folder. (To make the SHELL bootable USB disk, make sure      *
*         the bootX64.efi file¡¦s path must be                              *
*          ¡§FS0:\efi\boot\bootX64.efi¡¨)                                   *
*     3.  Please disable Secure Boot options in Security menu and check     *
*         CSM options is disabled in Startup menu before flash BIOS.        *
*     4.  Run UEFI mode and boot to USB disk. (Press F12 to UEFI USB disk). *
*     5.  System will auto flash via startup.nsh                            *
*     6.  Update may take up to 3 minutes. Do not power off or restart the  *
*         system during this procedure!                                     *
*     7.  After the flash update is complete. Don't forget to remove the    *
*         flash device and press ALT+CTRL+DEL to restart system.            *
*                                                                           *
*                                                                           *
*****************************************************************************

