
 --CONTENTS--
 1 - Installation Instructions
 2 - Flash under Operating System
 

*****************************************************************************
*                       1. Installation Instructions                        *
*                                                                           *
*     This flash under operating system (64-bit) utility provides           *
*     the ability to update the system BIOS from a Windows application.     *
*                                                                           *
*     The utility may be downloaded from the internet and unpacked          *
*     Please follow steps in section 2 to launch the Windows based flash    *
*     application to update your system BIOS.                               *
*                                                                           *
*                                                                           *
*****************************************************************************


*****************************************************************************
*                     2. Flash Under Operating System                       *
*                                                                           *
*     1.  Please make note of any settings you have changed in the BIOS     *
*         Setup utility. They may have to be re-entered after updating      *
*         the BIOS.                                                         *
*                                                                           *
*     2.  Click on the Start button and type cmd.exe,  Right-click on       *
*         the cmd.exe application and select run as administrator to        *
*         open the Command Prompt with Administrator privilege.             *
*                                                                           *
*     3.  In the "Command Prompt" window, change to the directory where the *
*         above files were extracted.                                       *
*                                                                           *
*     4.  Enter the command "flash64.cmd" and press the Enter key to start  *
*         the flashing process.                                             *
*                                                                           *
*     5.  The update may take up to 2 minutes. Do not power off or restart  *
*         the system during this procedure!                                 *
*                                                                           *
*     6.  When the BIOS update process ends, please restart system manually.*
*                                                                           *
*     7.  The BIOS update process ends with above six steps.                *
*                                                                           *
*****************************************************************************

